
**Online Blinds Order or Quote Form**



**Colourbond Corrugated Window Awnings**

www.onlineblinds.com.au

Phone: 1800 350 221

Mobile: 0417 622 171

Email: orders@onlineblinds.com.au

**How to order :**

1. Complete the details in the form below and email to orders@onlineblinds.com.au
2. We will confirm your order/quote with an email to you including delivery and payment options.
3. When pricing always go up to next measurement if in between eg: 2100mm wide price out at 2200mm

**Unfortunately we do not accept orders over the phone**

**Order Form:**

The corrugated roof sheets are available in Zincalume and Colourbond colours

The aluminium frames (top and bottom rails) and sides are available in Black, White and Colourbond colours.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date:** | | | | | | | | | | Awnings are custom made to your width measurement - maximum width of 3000mm with a fixed size of 750mm high x 645mm projection x 750mm skin @ 33 degrees angle  *Width measurement is overall including the 80mm gable roll*  *Eg: Awning Size 2200mm wide – fit size 2120mm*  *Fit size measurement is the outside measurement for the aluminium frame including the 40mm angle for fitting.* |
| **Name:** | | | | | | | | | |  |
| **Delivery Address:** | | | | |  | | | | |  |
| **Postcode:** | | | | |  |
| **Phone:** | | | | |  | | | | |  |
|  | | | | |  | | | | |  |
| **Email:** | | | | | | | | | |  |
|  | | | | | | | | | |  |
| AWNING  WIDTH in mm | CORRUGATED  STANDARD  COLOUR | CORRUGATED  SMALL/MINI  COLOUR | ALUMINIUM  FRAME  COLOUR | STANDARD  OPEN SIDES/ENDS | | CURVED  OPEN SIDES/ENDS | ALUMINIUM STATTED  SIDES/ENDS | ALUMINIUM  CURVED SLATTED SIDES/ENDS |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |
|  |  |  |  |  | |  |  |  |  | |

**How to measure**

***Wall with cladding -*** *brackets and end must be mounted to studs. - normally studs*

*are each side of window. Measure width of window (making sure of a flush fit to wall) then add on an extra 200mm to window width this will allow for the 40mm angle on side and gable roll eg 1810mm window would be awning width 2010mm.*

***Brick masonery fixing -*** *width of window plus 300mm minimum this allows for brick fixing approximately 70mm in frame edge of brick.*


*Wider is better (window width plus 400mm) No drills plug or dyna bolts supplied for brick fix.*

***Timber fix -*** *This will depend on the timber if in doubt fix same as cladding. When timber is good can be same as brick fix.*

***Standard casement window*** *approximately 450mm mounting height should be 250mm above window****.***

***Mounting height of awning will depend on head height and window style - sliding and with casement check mounting with the window open.***

***For installation over a hinged door allow 400mm above door for swing out of door.***



**Awnings are delivered flat packed with installation & assembly instructions and all the necessary brackets, screws etc ready for you to install for a timber & brick fit. Please specify for a steel fit. Wall plugs are not supplied for brickwork.**

*On placing your order full payment is required before we can proceed with your order. Confirmation email of your order will then be sent to you. Manufacturing of your order should be approximately 4 to 6 weeks. We accept Master & Visa Cards by phone or emailed and Direct Deposit as payment.*

***Freight Charges - Please provide Post Code for a delivery quote:***

***Free Delivery to Brisbane - please see areas below:***

***Brisbane Zone – Postcodes : 4000 to 4208; 4500 to 4511 & 4520***

*For all other areas please contact Online Blinds for a delivery quote.*

*All deliveries are door to door however in some regional areas we can arrange delivery to the nearest freight depot for you to collect.*

*All items are sent with Insurance and Tracking*