**Auto Lock Arm Retractable Awning**

**Online Blinds Order/Quote Form**

www.onlineblinds.com.au

Phone: 1800 350 221

Mobile: 0417 622 171

Email: orders@onlineblinds.com.au

***Blinds are custom made to your exact measurements provided – no standard sizes or pre-made blinds***

***Unfortunately we do not accept orders over the phone***

**How to Order:**

1. Measure the Width and Drop (Overall size as WIDTH PIN MEASUREMENT (outside bracket to outside bracket) – Skin DROP includes 150mm valance) Awnings are only suitable for Face Fit (outside fit)
2. Available fabrics – Barrington & Brella Canvas, Docril & Sattler Acrylic, Outlook Mode Colours, Privacy, Textures, Visiontex, Vistaweave & Atmosphere meshes – Straight Valance only available for mesh.

**(refer to the fabric link on home page to view fabric pdf files)**

Hood standard colours – White, Black, Primrose/Classic Cream, Stoney Beige/Paperbark & Anvil/Ironstone We are able to powdercoat Colourbond colours at an extra cost.

1. Complete the details in the form below and email to [orders@onlineblinds.com.au](mailto:orders@onlineblinds.com.au). If unable to download and complete form, please email your information.
2. We will confirm your order/quote by email to you including delivery and payment options.

When pricing always go up to next measurement if in between eg: 2200mm wide price out at 2350mm

**Order/Quote Form:**

|  |  |
| --- | --- |
| **Date:** | |
| **Name:** | |
| **Delivery Address:** |  |
| **Postcode:** |
| **Phone:** | **Fax:** |
| **Email:** | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Blind** | | | | | |  | | |
| **WIDTH** | **DROP** | **FABRIC CODE AND COLOUR** | **HOOD COLOUR** | **300MM ARMS** | **150MM ARMS** | **WAVEY VALANCE** | **STRAIGHT VALANCE** |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  | | | | | | | | |

**Awnings are delivered to your door fully assembled with installation instructions and all the necessary brackets, screws etc ready for you to install for a timber fit also suitable for brick fit. Please specify for a steel fit. Wall plugs are not supplied for brickwork.**

*On placing your order full payment is required before we can proceed with the order. Confirmation email for your order will then be sent to you. Manufacturing of your order should be approximately 2 to 4 weeks. We accept Master & Visa Cards by phone or emailed and Direct Deposit as payment.*

**Freight Charges**

Please provide Suburb/Post Code for a delivery quote:

**We offer free delivery to Brisbane, please see areas below:**

Brisbane Zone – Post Codes : 4000 to 4208; 4500 to 4511 & 4520

For all other areas please contact Online Blinds for a delivery quote.

All deliveries are door to door however in some regional areas we can arrange delivery to the nearest freight depot for you to collect. All items are sent with Insurance and Tracking.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  | | | |
|  | | | |

**Handy Hints:**

* You will need a good tape measure (metal ones are the best) all measurements are to be in mm (2120mm)
* When measuring always look out for things like down pipes, windows that open outwards or if the awning is in the way of a walk way.

Awnings are only suitable for FACE FIT (outside mount) and to be installed at ground level

**WIDTH**: Measure window width and add a minimum of 150mm to each side where possible.   
**DROP**: Take a point 150mm above window, measure from the point to required drop.

(Overall size as WIDTH PIN MEASUREMENT (outside bracket to outside bracket) – Skin DROP includes 150mm valance)

All our products are custom made to your measurements, **MANUFACTURED IN AUSTRALIA** and we use Australian made components where possible.

We use only the best quality materials in manufacturing of all our products. We are happy to provide a 100% manufacturer’s guarantee, where we replace or repair any faulty materials or workmanship. We will not be held responsible for the intentions of where and how our products are installed. We offer a 2 years warranty on the manufacturing and all components of our products.

